**Lecture 1 – Introduction, types of textile measurements**

|  |
| --- |
| Basic textile unit is fineness (linear density) T [tex]. Its size is [g/km]. What size has the unit in basic SI units [kg/m]? |
| a) dtexb) ktexc) Mtex |

|  |
| --- |
| Convert derived SI units to basic SI units:Example: [Pa] = [kg.m-1.s-2] |
| a) Energy E [J]b) Power P [W]c) Force F [N]d) Dynamic viscosity η [Pa.s]e) Specific strength Fp [N/tex]f) Voltage U [V] |

|  |
| --- |
| Define internal material properties? |
|  |

|  |
| --- |
| Define product properties? |
|  |

**Lecture 2 – Sensors, data processing, analysis, data presentation**

|  |
| --- |
| What is the use of following parts of measuring system: |
| a) Sensorb) Converterc) Receiver |

|  |
| --- |
| Calculate parameters below for given data (diameter of PES fibers in μm):  |
| a) Meanb) Modusc) Mediand) Variancee) Standard deviationf) Coefficient of variation | Using lanameter we obtained following parameters of PES fibres diameter in μm: 20,1; 22,8; 19,6; 18,9; 20,1; 23,2; 20,6; 21,2; 21,0; 20,6; |

|  |
| --- |
| What will be the correct interpretation of results from paremeters below? |
| $$\overbar{T }\left[dtex\right]=6,549$$s2 = 1,686445071 | a) 6,549 ± 1,53501 dtexb) 6,55 ± 1,298632 dtexc) 6,5 ± 1,2 dtexConvert the results into [tex] units |

|  |
| --- |
| Draw the histogram for data set below (length of fibers): |
|

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| j | ljd - ljh [mm] | lj [mm] | nj | fj |
|  1 | 5-15 | 10 | 10 |  |
| 2 | 15-25 | 20 | 13 |  |
| 3 | 25-35 | 30 | 20 |  |
| 4 | 35-45 | 40 | 27 |  |
| 5 | 45-55 | 50 | 30 |  |

**n = Σnj = 100 !** |

**Lecture 3 – Sampling, nuber of measurements**

|  |
| --- |
| Explain the term "random selection": |
|  |

|  |
| --- |
| What is the method of fiber selection from woven fabric according to ISO Standards?  |
|  |

|  |
| --- |
| How we estimate number of measurements? |
|  |

|  |
| --- |
| How we estimate climatic conditions for measurement? What are normal laboratory conditions? |
|  |

|  |
| --- |
| Why we pre-dry and condition textile specimen? |
|  |

**Lecture 4 – Moisture sorption**

|  |
| --- |
| Define term "Fiber sorption properties". What does mean hydrophobic a hydrophilic? |
|  |

|  |
| --- |
| What does mean "Commercial moisture regain", why we need to define it? |
|  |

|  |
| --- |
| How we estimate moisture content in fibers? |
|  |

|  |
| --- |
| How is defined relative air humidity? What is dew point, how is linked to temperature? |
|  |

**Lecture 5 – Geometry of fibers**

|  |
| --- |
| Derive relation between fineness and diameter of circular fibers. Describe quantities and units used for calculation: |
|  |

|  |
| --- |
| How is defined fiber length? Describe the method for measurement of lengthes of fibers embedded in staple yarn? |
|  |

|  |
| --- |
| How You estimate Specific surface of fibers **Sp [m2/kg]** for circular fiber with fineness T = 3, 6, and 9 dtex? |
|  |

|  |
| --- |
| How is defined equivalent fiber diameter? Can You use it for description of shape of fiber cross-section? |
|  |